; Generated by DriverWizard v9.00 - http://www.jungo.com.
; Installation file (.inf) for "CAS3 PLUS Interface" device
; Copyright (c) 2007 Duolabs
;
; You can create a customized version of this file
; by modifying the specified sections.
;
; Refer to Windows DDK documentation for more information on INF files
;

; Version Information
; -------------------
[Version]
Signature="$CHICAGO$"  ; Represents all Windows OS's
Provider=%jun%
; For WHQL, you should obtain a catalog signed by Microsoft Hardware Compatibility Labs
; CatalogFile=wd900.cat
DriverVer=04/06/2007, 9.0.0

Class=Jungo
ClassGuid={c671678c-82c1-43f3-d700-0049433e9a4b}

; Driver Information
; ------------------
[Manufacturer]
; You may modify the manufacturer name by changing the Mfg variable in the [Strings]
; section in this INF file.
%Mfg%=DeviceList,NTamd64

; x86 platform, Win9x, Windows 2000 and later
[DeviceList]
"CAS Interface 2 USB"=Install, USB\VID_0547&PID_2131
"CAS Interface 2 USB"=Install, USB\VID_0547&PID_1004
"CAS Interface 2 USB"=Install, USB\VID_0547&PID_1005
"CAS Interface 2 USB"=Install, USB\VID_0547&PID_1002
"CAS Interface 2 USB"=Install, USB\VID_0547&PID_3121

"Dynamite"=Install, USB\VID_0547&PID_1010

"Dynamite PLUS USB"=Install, USB\VID_04B4&PID_1111
"Dynamite PLUS v.2.0 USB"=Install, USB\VID_04B4&PID_1112

"CAS2 PLUS USB"=Install, USB\VID_04B4&PID_2223
"CAS2 PLUS v.2.0 USB"=Install, USB\VID_04B4&PID_2225

"CAS Interface 3 USB"=Install, USB\VID_04B4&PID_2222
"CAS Interface 3 USB"=Install, USB\VID_04B4&PID_8613
"CAS Interface 3 USB"=Install, USB\VID_04B4&PID_6473
"CAS Interface 3 USB"=Install, USB\VID_04B4&PID_3232

; x64 platform, Windows XP x64 edition and later
[DeviceList.NTamd64]
"CAS Interface 2 USB"=Install, USB\VID_0547&PID_2131
"CAS Interface 2 USB"=Install, USB\VID_0547&PID_1004
"CAS Interface 2 USB"=Install, USB\VID_0547&PID_1005
"CAS Interface 2 USB"=Install, USB\VID_0547&PID_1002
"CAS Interface 2 USB"=Install, USB\VID_0547&PID_3121

"Dynamite"=Install, USB\VID_0547&PID_1010

"Dynamite PLUS USB"=Install, USB\VID_04B4&PID_1111
"Dynamite PLUS v.2.0 USB"=Install, USB\VID_04B4&PID_1112

"CAS2 PLUS USB"=Install, USB\VID_04B4&PID_2223
"CAS2 PLUS v.2.0 USB"=Install, USB\VID_04B4&PID_2225

"CAS Interface 3 USB"=Install, USB\VID_04B4&PID_2222
"CAS Interface 3 USB"=Install, USB\VID_04B4&PID_8613
"CAS Interface 3 USB"=Install, USB\VID_04B4&PID_6473
"CAS Interface 3 USB"=Install, USB\VID_04B4&PID_3232

; Installation Section
; --------------------
[Install]  ; Installation script for Windows 98/Me
CopyFiles=FilesToCopy
AddReg=UpDateRegistry

[Install.NT]  ; Installation script for Windows 2000 and later
CopyFiles=FilesToCopy
AddReg=UpDateRegistry

[FilesToCopy]
; To copy windrvr6.sys upon installation remove the ';' from the start of the following line
;windrvr6.sys ,,,0x40  ; 0x40 == COPYFLG_OVERWRITE_OLDER_ONLY

[ClassInstall]  ; Register a new class in Windows 98/Me
AddReg=UpDateRegistry

[ClassInstall32]  ; Register a new class in Windows 2000 and later
AddReg=UpDateRegistry

[UpDateRegistry]
HKR,,,,Jungo
HKR,,Icon,,-5
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,, windrvr6.sys

[ControlFlags]
ExcludeFromSelect = *  ; Remove all devices listed in this INF file from certain user 
;    interface displays, from which a user is expected to select a particular device 
;    for installation.

[PreCopySection]
HKR,,NoSetupUI,,1

; Defining WinDriver6 Service
; ---------------------------
[Install.NT.Services]
Addservice=WinDriver6, 0x00000002, Service_Info

[Service_Info]
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\windrvr6.sys

; Source File Information
; -----------------------
[SourceDisksFiles]
windrvr6.sys=1  ; This indicates that the windrvr6.sys file is located on
    ; disk number 1 of "Duolabs Installation disks" set.

[SourceDisksNames]
1="Duolabs Installation Disk",,  ; This indicates that disk number 1
    ; has the label "Duolabs Installation Disk". The installer will
    ; search for windrvr6.sys in this disk.

[DestinationDirs]
DefaultDestDir=10, System32\Drivers  ; The location to which the windrvr6.sys
    ; file will be copied (10 translates to the correct Windows directory
    ; on the target machine).


;---------------------------------------------------------------;

[Strings]
jun="Jungo LTD."
Mfg="Duolabs"

