;=============================================================== 
; [TGL176G.INF] 
; Revision 1.0   June-13-2008
; Copyright(c)2008 TriGem Computer, Inc.,All Rights Reserved.
;===============================================================
;
[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%TG%
CatalogFile=TGL176G.cat
DriverVer=06/13/2008,1.0

[ControlFlags]
ExcludeFromSelect.NT=Monitor\GSM44A3
ExcludeFromSelect.NT=Monitor\GSM44A4

[DestinationDirs]
DefaultDestDir = 11
TGL176G_Analog.CopyFiles = 23
TGL176G_Digital.CopyFiles = 23

[SourceDisksNames]
1=%DiskName%,,,

[SourceDisksFiles]
TGL176G.ICM=1

[Manufacturer]
%TG%=TG,NTamd64

[TG]
%TGL176G_Analog%=TGL176G_Analog.Install,Monitor\GSM44A3
%TGL176G_Digital%=TGL176G_Digital.Install,Monitor\GSM44A4

[TG.NTamd64]
%TGL176G_Analog%=TGL176G_Analog.Install,Monitor\GSM44A3
%TGL176G_Digital%=TGL176G_Digital.Install,Monitor\GSM44A4

[TGL176G_Analog.Install]
DelReg=DEL_CURRENT_REG
AddReg=TGL176G_Analog.AddReg,1280,DPMS
CopyFiles=TGL176G_Analog.CopyFiles

[TGL176G_Digital.Install]
DelReg=DEL_CURRENT_REG
AddReg=TGL176G_Digital.AddReg,1280,DPMS
CopyFiles=TGL176G_Digital.CopyFiles

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[1280]
HKR,,MaxResolution,,"1280,1024"

[DPMS]
HKR,,DPMS,,1

[TGL176G_Analog.AddReg]
HKR,"MODES\1280,1024",Mode1,,"30.0-83.0,56.0-75.0,+,+"
HKR,,PreferredMode,,"1280,1024,60"
HKR,,ICMprofile,0,"TGL176G.ICM"

[TGL176G_Digital.AddReg]
HKR,"MODES\1280,1024",Mode1,,"30.0-71.0,56.0-75.0,+,+"
HKR,,PreferredMode,,"1280,1024,60"
HKR,,ICMprofile,0,"TGL176G.ICM"

[TGL176G_Analog.CopyFiles]
TGL176G.ICM

[TGL176G_Digital.CopyFiles]
TGL176G.ICM

[Strings]
DiskName="TG Monitor Profiles Installation Disk"
TG="TG"
TGL176G_Analog="TG TGL 176G(Analog)"
TGL176G_Digital="TG TGL 176G(Digital)"