; *************************************************************************
; *************************************************************************
; **	Filename:		mxtBootBridge.inf
; **	Abstract:		INF for Driver Framework for mxtBootBridge Driver
; **	Target OS:		Win8.0, Win8.1, Win10
; **	Arch:			x86, amd64
; **	Last Updated:	July 30, 2015 (Vers 10.1.14.10130)
; **
; **	Copyright (c) Atmel Corporation.  All rights reserved.	
; **
; *************************************************************************
; *************************************************************************


[Version]
Signature		="$WINDOWS NT$"
Class			= System
ClassGuid		= {4D36E97D-E325-11CE-BFC1-08002BE10318}
Provider		= %VendorName%
CatalogFile		= mxtBootBridge.cat
DriverVer=07/30/2015,10.1.14.10130

[DestinationDirs]
DefaultDestDir = 12

; *************************************************************************
; **	Specify install disks
; *************************************************************************

[SourceDisksNames]
1= %DiskName%,,,""

[SourceDisksFiles]
mxtBootBridge.sys = 1,,

[DefaultInstall]
mxtBootBridge.sys = 1,,

; *************************************************************************
; **	Device Section
; *************************************************************************

[mxtBootBridge_Device.NT]	
CopyFiles=mxtBootBridgeSysFiles.NT.CopyFiles

[mxtBootBridgeSysFiles.NT.CopyFiles]
mxtbootbridge.sys

; *************************************************************************
; **	Manufacturer Section
; *************************************************************************


[Manufacturer]
%VendorName% = Atmel,NTx86.6.2,NTamd64.6.2,NTx86.6.3,NTamd64.6.3,NTx86.10.0,NTamd64.10.0

; Install on Windows 8.0, Windows 8.1, and Windows 10

[Atmel.NTx86.6.2]
%mxtBootBridge.DeviceDesc%=mxtBootBridge_Device, ACPI\ATML2000

[Atmel.NTamd64.6.2]
%mxtBootBridge.DeviceDesc%=mxtBootBridge_Device, ACPI\ATML2000

[Atmel.NTx86.6.3]
%mxtBootBridge.DeviceDesc%=mxtBootBridge_Device, ACPI\ATML2000

[Atmel.NTamd64.6.3]
%mxtBootBridge.DeviceDesc%=mxtBootBridge_Device, ACPI\ATML2000

[Atmel.NTx86.10.0]
%mxtBootBridge.DeviceDesc%=mxtBootBridge_Device, ACPI\ATML2000

[Atmel.NTamd64.10.0]
%mxtBootBridge.DeviceDesc%=mxtBootBridge_Device, ACPI\ATML2000

[mxtBootBridge_Device.NT.Services]
AddService = mxtBootBridge,%SPSVCINST_ASSOCSERVICE%, mxtBootBridge_Service_Inst

[mxtBootBridge_Service_Inst]

DisplayName    = %mxtBootBridge.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START 
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\mxtBootBridge.sys
LoadOrderGroup = Extended Base

[Strings]
WINDOWS_DIR            = 10 ; %windir%
DRIVERS_DIR            = 12 ; %windir%\system32\drivers
SPSVCINST_ASSOCSERVICE	 = 0x00000002
VendorName				= "Atmel Corporation"
InstallDisk1            = "mxtBootBridge Peripheral Installation Disk #1"
DiskName				= "mxtBootBridge Installer"
mxtBootBridge.DeviceDesc = "maxTouch I2C Boot Bridge Peripheral Driver"
mxtBootBridge.SVCDESC    = "maxTouch I2C Boot Bridge Peripheral Service"
