; CH432_4S.INF
; Driver for CH432 (PCI=>Serials) chip V1.0
; For Windows XP/VISTA
; Copyright (C) WCH 2001-2007

[Version]
Signature="$Windows NT$"
Class=MultiFunction
ClassGUID={4d36e971-e325-11ce-bfc1-08002be10318}
Provider=%WinChipHead%
DriverVer=07/01/2007

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%WinChipHead%=WinChipHead

[WinChipHead]
%WinChipHead_PORT_MS%=WinChipHeadMS_inst,pci\ven_4348&dev_5049
%WinChipHead_PORT_MS%=WinChipHeadMS_inst,pci\ven_4348&dev_5049&subsys_00000000

[WinChipHeadMS_inst.NT]
Include = mf.inf
Needs = MFINSTALL.mf

[WinChipHeadMS_inst.NT.HW]
AddReg=WinChipHeadMS_inst.NT.RegHW

[WinChipHeadMS_inst.NT.Services]
Include = mf.inf
Needs = MFINSTALL.mf.Services
       
[WinChipHeadMS_inst.NT.RegHW]
HKR,Child0000,HardwareID,,MF\PCI5049_COM_0
HKR,Child0000,ResourceMap,1,04
HKR,Child0000,VaryingResourceMap,1,00,00,00,00,00,08,00,00,00
HKR,Child0001,HardwareID,,MF\PCI5049_COM_1
HKR,Child0001,ResourceMap,1,04
HKR,Child0001,VaryingResourceMap,1,00,08,00,00,00,08,00,00,00
HKR,Child0002,HardwareID,,MF\PCI5049_COM_2
HKR,Child0002,ResourceMap,1,04
HKR,Child0002,VaryingResourceMap,1,00,10,00,00,00,08,00,00,00
HKR,Child0003,HardwareID,,MF\PCI5049_COM_3
HKR,Child0003,ResourceMap,1,04
HKR,Child0003,VaryingResourceMap,1,00,18,00,00,00,08,00,00,00
;if the card is 6 serials,delete the ';' at the begin of following 6 lines
;if the card is 8 serials,delete the ';' at the begin of following 12 lines
;HKR,Child0004,HardwareID,,MF\PCI5049_COM_4
;HKR,Child0004,ResourceMap,1,04
;HKR,Child0004,VaryingResourceMap,1,00,20,00,00,00,08,00,00,00
;HKR,Child0005,HardwareID,,MF\PCI5049_COM_5
;HKR,Child0005,ResourceMap,1,04
;HKR,Child0005,VaryingResourceMap,1,00,28,00,00,00,08,00,00,00
;HKR,Child0006,HardwareID,,MF\PCI5049_COM_6
;HKR,Child0006,ResourceMap,1,04
;HKR,Child0006,VaryingResourceMap,1,00,30,00,00,00,08,00,00,00
;HKR,Child0007,HardwareID,,MF\PCI5049_COM_7
;HKR,Child0007,ResourceMap,1,04
;HKR,Child0007,VaryingResourceMap,1,00,38,00,00,00,08,00,00,00


[Strings]
WinChipHead= "wch.cn"
WinChipHead_PORT_MS = "PCI =>SERIAL"


