;
; Copyright (c) Fujitsu Frontech All rights reserved.
;
[Version]
Signature="$CHICAGO$"
Class=USB
ClassGuid={36fc9e60-c465-11cf-8056-444553540000}
provider=%MfgName%
DriverVer=02/28/2006,2.1.0.10
Catalogfile=ctusbdr.cat

[Manufacturer]
%MfgName%=SECTION_0

;[ControlFlags]
;ExcludeFromSelect=*

[SECTION_0]
%USB\VID_04C5&PID_1104.DeviceDesc%=ctusbdr.Dev, USB\VID_04C5&PID_1104
;%USB\VID_2730&PID_0FFF.DeviceDesc%=ctusbdr.Dev, USB\VID_2730&PID_0FFF

;[PreCopySection]
;HKR,,NoSetupUI,,1

[DestinationDirs]
ctusbdr_COPYFILES = 10,System32\Drivers

[ctusbdr.Dev]
CopyFiles=ctusbdr_COPYFILES
AddReg=ctusbdr.AddReg

[ctusbdr.Dev.NT]
CopyFiles=ctusbdr_COPYFILES
AddReg=ctusbdr.AddReg

[ctusbdr.AddReg]

[ctusbdr_COPYFILES]
ctusbdr.sys

[ctusbdr.Dev.NT.HW]
AddReg=ctusbdr.Dev.NT.HW.AddReg

[ctusbdr.Dev.NT.HW.AddReg]
HKR,,"EndPointCaps",0x00010001,3
HKR,,"DebugLevel",0x00010001,0x3
HKR,,"RawDump",0x00010001,0
HKR,,"RxReqSize",0x00010001,64
HKR,,"TxReqSize",0x00010001,64
HKR,,"CtlPollPeriod",0x00010001,-1
HKR,,"RxPollPeriod",0x00010001,0
HKR,,"TxKickThreshold",0x00010001,64
HKR,,"LatencyTimer",0x00010001,16

[ctusbdr.Dev.NT.Services]
Addservice = ctusbdr,2,ctusbdr.AddService

[ctusbdr.AddService]
DisplayName    = %ctusbdr.SvcDesc%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\ctusbdr.sys
LoadOrderGroup = Base

[SourceDisksFiles]
ctusbdr.sys=1

[SourceDisksNames]
1=%InstallDiskName%

[Strings]
MfgName="Fujitsu Frontech"
USB\VID_04C5&PID_1104.DeviceDesc="Fujitsu CT10/11 Printer Communication Port"
;USB\VID_2730&PID_0FFF.DeviceDesc="Fujitsu Frontech Virtual Communication Port"
ctusbdr.SvcDesc="USB Driver for Virtual Communication Port"
InstallDiskName="Virtual Communication Port Setup Disk"
