;/*++
;
; Copyright (c) 2012  by KYOCERA Corporation
;
;--*/

[Version]
Signature = "$WINDOWS NT$"
Class     = AndroidUsbDeviceClass
ClassGuid = {3F966BD9-FA04-4ec5-991C-D326973B5128}
Provider  = %KYOCERA%
DriverVer=04/23/2013,3.0.0.2
CatalogFile=kc02us_adb.cat

; ================= Device section =====================
;
; This section seems to be required for WinUsb driver installation.
; If this section is removed the installer will report an error
; "Required section not found in INF file".
;
[ClassInstall32]
Addreg = AndroidWinUsbClassReg

[AndroidWinUsbClassReg]
HKR,,,0,%ClassName%
HKR,,Icon,,-1

[Manufacturer]
%MfgName%=Kyocera, NTx86, NTamd64

[Kyocera.NTx86]
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_051B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0524&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_052A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_052C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0546&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0548&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0556&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0557&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_056E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_056F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0558&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0559&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_055A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_055B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0572&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0573&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_057f&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0580&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_058D&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_058E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_058f&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0590&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0594&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0595&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0596&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0597&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0598&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0599&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_059D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_059E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05A8&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05A9&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05aa&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05ab&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05AF&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05B0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05dc&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05dd&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05df&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e0&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e3&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e4&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e5&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e6&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e7&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e9&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05ea&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05eb&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05ec&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05ed&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05ee&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05ef&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05f0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05f1&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05f2&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05f3&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05f4&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05f5&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05f6&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05f7&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05f8&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0702&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0703&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0704&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0705&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0706&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0707&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0708&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0709&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_070a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_070b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_070c&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_070d&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_070e&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_070f&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0710&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0711&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0712&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0713&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0714&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0715&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0716&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0717&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0718&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0719&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_071b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_071c&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_071d&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_071e&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_071f&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0720&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0721&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0722&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0723&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0724&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0725&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0726&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0727&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0728&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0729&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_072a&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_072b&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_072c&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_072d&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_072e&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_072f&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0730&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0731&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0732&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0734&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0735&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0736&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0737&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0738&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0739&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_073a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_073b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_073c&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_073d&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_073e&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_073f&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0740&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0741&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0742&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0743&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0744&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0745&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0746&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0747&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0748&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0749&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_074a&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_074b&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_074c&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_074d&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_074f&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0750&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0751&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0752&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0753&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0754&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0755&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0756&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0757&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0758&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0759&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_075a&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_075b&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_075c&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_075d&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_075e&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_075f&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0760&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0761&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0762&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0763&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0764&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0765&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0766&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0790&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0791&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0792&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0793&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0794&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0795&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0796&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0797&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0798&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0799&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_079a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_079b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_079c&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_079d&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_079e&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_079f&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_07ed&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_07ee&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_07ef&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_07f0&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_07f1&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_07f2&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_07f3&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_07f4&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0822&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0823&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0824&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0825&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0826&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0827&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0828&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0829&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_082a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_082b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_082c&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_082d&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_082e&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_082f&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0830&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0831&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0832&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0833&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0834&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0835&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0836&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0837&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0838&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0839&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_083a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_083b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_083c&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_083d&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_083e&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_083f&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0840&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0841&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_084b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_084d&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_084f&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0851&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0853&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0855&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0857&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0859&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_085b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_085d&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_085f&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0861&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0863&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0865&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0867&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0869&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_086b&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_086d&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_086f&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0871&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0873&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0875&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0877&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0879&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_087c&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_087e&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0880&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0882&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0884&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0886&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0888&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_088a&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_088c&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_088e&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0890&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0892&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0894&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0896&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0898&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_089a&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_089c&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_089e&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08a0&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08a2&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08a4&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08a6&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08a8&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08aa&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08cd&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08ce&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08d0&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08d1&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08d2&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08d3&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08d4&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08d5&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08d6&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08d7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08d8&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08d9&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08da&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08db&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08dc&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08dd&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0992&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0993&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0994&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0995&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0996&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0997&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0998&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0999&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08de&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08df&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08e0&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08e1&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08e2&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08e3&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08e4&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08e5&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08e6&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08e7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08e9&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08ea&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08ec&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08ed&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08ee&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08ef&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08f0&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08f1&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08f2&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08f3&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08f4&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08f5&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08f6&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08f7&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08f8&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08f9&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08fa&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08fb&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08fc&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08fd&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08fe&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08ff&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0900&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0901&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0902&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0903&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0922&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0923&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0924&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0925&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0926&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0927&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0928&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0929&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_092a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_092b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_092c&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_092d&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_092e&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_092f&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0930&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0931&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0932&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0933&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0934&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0935&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0936&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0937&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0938&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0939&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_093a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_093b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_093c&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_093d&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_093e&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_093f&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0940&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0941&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0944&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0945&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0946&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0947&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0948&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0949&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_094a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_094b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_094c&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_094d&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_094e&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_094f&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0950&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0951&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0952&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0953&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0954&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0955&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0956&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0957&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0958&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0959&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_095a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_095b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_095c&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_095d&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_095e&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_095f&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0960&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0961&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0962&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0963&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0970&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0971&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0972&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0973&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0974&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0975&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0976&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0977&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0978&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0979&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_097a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_097b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_097c&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_097d&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_097e&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_097f&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_099a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_099b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_099c&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_099d&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_099e&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_099f&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09a0&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09a1&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0980&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0981&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0982&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0983&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0984&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0985&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0986&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0987&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0988&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0989&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_098a&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_098b&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_098c&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_098d&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_098e&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_098f&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09ae&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09af&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09b0&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09b1&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09b2&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09b3&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09b4&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09b5&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09b6&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09b7&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0a8f&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0a91&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0a93&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0a95&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0a97&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0a99&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0a9b&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0a9d&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0a9f&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0aa1&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0aa3&MI_03

[Kyocera.NTamd64]
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_051B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0524&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_052A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_052C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0546&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0548&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0556&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0557&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_056E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_056F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0558&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0559&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_055A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_055B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0572&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0573&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_057f&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0580&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_058D&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_058E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_058f&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0590&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0594&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0595&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0596&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0597&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0598&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0599&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_059D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_059E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05A8&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05A9&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05aa&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05ab&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05AF&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05B0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05dc&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05dd&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05df&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e0&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e3&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e4&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e5&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e6&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e7&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e8&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e9&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05ea&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05eb&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05ec&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05ed&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05ee&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05ef&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05f0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05f1&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05f2&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05f3&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05f4&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05f5&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05f6&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05f7&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05f8&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0702&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0703&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0704&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0705&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0706&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0707&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0708&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0709&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_070a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_070b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_070c&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_070d&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_070e&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_070f&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0710&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0711&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0712&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0713&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0714&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0715&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0716&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0717&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0718&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0719&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_071b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_071c&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_071d&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_071e&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_071f&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0720&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0721&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0722&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0723&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0724&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0725&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0726&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0727&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0728&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0729&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_072a&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_072b&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_072c&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_072d&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_072e&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_072f&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0730&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0731&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0732&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0734&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0735&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0736&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0737&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0738&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0739&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_073a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_073b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_073c&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_073d&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_073e&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_073f&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0740&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0741&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0742&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0743&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0744&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0745&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0746&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0747&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0748&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0749&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_074a&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_074b&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_074c&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_074d&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_074f&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0750&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0751&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0752&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0753&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0754&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0755&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0756&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0757&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0758&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0759&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_075a&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_075b&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_075c&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_075d&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_075e&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_075f&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0760&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0761&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0762&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0763&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0764&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0765&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0766&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0790&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0791&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0792&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0793&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0794&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0795&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0796&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0797&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0798&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0799&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_079a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_079b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_079c&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_079d&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_079e&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_079f&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_07ed&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_07ee&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_07ef&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_07f0&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_07f1&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_07f2&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_07f3&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_07f4&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0822&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0823&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0824&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0825&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0826&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0827&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0828&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0829&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_082a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_082b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_082c&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_082d&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_082e&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_082f&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0830&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0831&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0832&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0833&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0834&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0835&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0836&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0837&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0838&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0839&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_083a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_083b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_083c&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_083d&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_083e&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_083f&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0840&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0841&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_084b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_084d&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_084f&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0851&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0853&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0855&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0857&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0859&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_085b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_085d&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_085f&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0861&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0863&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0865&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0867&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0869&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_086b&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_086d&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_086f&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0871&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0873&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0875&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0877&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0879&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_087c&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_087e&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0880&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0882&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0884&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0886&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0888&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_088a&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_088c&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_088e&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0890&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0892&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0894&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0896&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0898&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_089a&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_089c&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_089e&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08a0&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08a2&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08a4&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08a6&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08a8&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08aa&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08cd&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08ce&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08d0&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08d1&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08d2&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08d3&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08d4&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08d5&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08d6&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08d7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08d8&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08d9&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08da&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08db&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08dc&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08dd&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0992&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0993&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0994&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0995&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0996&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0997&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0998&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0999&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08de&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08df&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08e0&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08e1&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08e2&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08e3&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08e4&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08e5&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08e6&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08e7&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08e9&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08ea&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08ec&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08ed&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08ee&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08ef&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08f0&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08f1&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08f2&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08f3&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08f4&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08f5&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08f6&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08f7&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08f8&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08f9&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08fa&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08fb&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08fc&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08fd&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08fe&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_08ff&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0900&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0901&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0902&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0903&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0922&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0923&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0924&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0925&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0926&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0927&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0928&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0929&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_092a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_092b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_092c&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_092d&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_092e&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_092f&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0930&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0931&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0932&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0933&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0934&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0935&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0936&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0937&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0938&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0939&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_093a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_093b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_093c&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_093d&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_093e&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_093f&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0940&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0941&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0944&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0945&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0946&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0947&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0948&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0949&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_094a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_094b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_094c&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_094d&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_094e&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_094f&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0950&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0951&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0952&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0953&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0954&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0955&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0956&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0957&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0958&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0959&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_095a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_095b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_095c&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_095d&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_095e&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_095f&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0960&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0961&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0962&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0963&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0970&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0971&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0972&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0973&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0974&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0975&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0976&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0977&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0978&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0979&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_097a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_097b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_097c&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_097d&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_097e&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_097f&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_099a&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_099b&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_099c&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_099d&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_099e&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_099f&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09a0&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09a1&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0980&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0981&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0982&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0983&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0984&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0985&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0986&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0987&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0988&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0989&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_098a&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_098b&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_098c&MI_05
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_098d&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_098e&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_098f&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09ae&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09af&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09b0&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09b1&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09b2&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09b3&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09b4&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09b5&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09b6&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_09b7&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0a8f&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0a91&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0a93&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0a95&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0a97&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0a99&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0a9b&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0a9d&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0a9f&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0aa1&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0aa3&MI_03

[USB_Install]
Include = winusb.inf
Needs   = WINUSB.NT

[USB_Install.Services]
Include     = winusb.inf
AddService  = WinUSB,0x00000002,WinUSB_ServiceInstall

[WinUSB_ServiceInstall]
DisplayName     = %WinUSB_SvcDesc%
ServiceType     = 1
StartType       = 3
ErrorControl    = 1
ServiceBinary   = %12%\WinUSB.sys

[USB_Install.Wdf]
KmdfService = WINUSB, WinUSB_Install

[WinUSB_Install]
KmdfLibraryVersion = 1.9

[USB_Install.HW]
AddReg  = Dev_AddReg

[Dev_AddReg]
HKR,,DeviceInterfaceGUIDs,0x10000,"{F72FE0D4-CBCB-407d-8814-9ED673D0DD6B}"

[USB_Install.CoInstallers]
AddReg    = CoInstallers_AddReg
CopyFiles = CoInstallers_CopyFiles

[CoInstallers_AddReg]
HKR,,CoInstallers32,0x00010000,"WdfCoInstaller01009.dll,WdfCoInstaller","WinUSBCoInstaller2.dll"

[CoInstallers_CopyFiles]
WinUSBCoInstaller2.dll
WdfCoInstaller01009.dll

[DestinationDirs]
CoInstallers_CopyFiles=11

[SourceDisksNames]
1 = %DISK_NAME%,,,\i386
2 = %DISK_NAME%,,,\amd64

[SourceDisksFiles.x86]
WinUSBCoInstaller2.dll  = 1
WdfCoInstaller01009.dll = 1

[SourceDisksFiles.amd64]
WinUSBCoInstaller2.dll  = 2
WdfCoInstaller01009.dll = 2

[Strings]
KYOCERA                     = "KYOCERA Corporation"
MfgName                     = "KYOCERA Corporation"
SingleAdbInterface          = "Android ADB Interface"
CompositeAdbInterface       = "Android Composite ADB Interface"
SingleBootLoaderInterface   = "Android Bootloader Interface"
WinUSB_SvcDesc              = "Android USB Driver"
DISK_NAME                   = "Android WinUsb installation disk"
ClassName                   = "Android Phone"

