;
; Android WinUsb driver installation.
;
[Version]
Signature           = "$Windows NT$"
Class               = AndroidUsbDeviceClass
ClassGuid           = {3F966BD9-FA04-4ec5-991C-D326973B5128}
Provider            = %ProviderName%
DriverVer           = 11/25/2021,12.0.0.0
CatalogFile.NTx86   = androidwinusb86.cat
CatalogFile.NTamd64 = androidwinusba64.cat
PnpLockdown         = 1
;
; This section seems to be required for WinUsb driver installation.
; If this section is removed the installer will report an error
; "Required section not found in INF file".
;
[ClassInstall32]
Addreg = AndroidWinUsbClassReg

[AndroidWinUsbClassReg]
HKR,,,0,%ClassName%
HKR,,Icon,,-1

[Manufacturer]
%ProviderName% = Google, NTx86, NTamd64

[Google.NTx86]
;Qualcomm SURF/FFA
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1200&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1201&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1203&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1204&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1206&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1208&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1212&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1216&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1217&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1221&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1222&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1223&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1230&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1231&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1232&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1234&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1235&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1260&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1261&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1262&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1040&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1041&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1042&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1043&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1045&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1050&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1051&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1052&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1053&MI_01
%CompositeAdbInterface_cust_1054% = USB_Install, USB\VID_1BC7&PID_1054&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1055&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1056&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1057&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1058&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1060&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1061&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1062&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1063&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1070&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1071&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1072&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1073&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1075&MI_00

%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_D00D

[Google.NTamd64]
;Qualcomm SURF/FFA
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1200&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1201&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1203&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1204&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1206&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1208&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1212&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1216&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1217&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1221&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1222&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1223&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1230&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1231&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1232&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1234&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1235&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1260&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1261&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1262&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1040&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1041&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1042&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1043&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1045&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1050&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1051&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1052&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1053&MI_01
%CompositeAdbInterface_cust_1054% = USB_Install, USB\VID_1BC7&PID_1054&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1055&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1056&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1057&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1058&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1060&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1061&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1062&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1063&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1070&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1071&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1072&MI_03
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1073&MI_01
%CompositeAdbInterface% = USB_Install, USB\VID_1BC7&PID_1075&MI_00

%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_D00D

[USB_Install]
Include = winusb.inf
Needs   = WINUSB.NT

[USB_Install.Services]
Include     = winusb.inf
AddService  = WinUSB,0x00000002,WinUSB_ServiceInstall

[WinUSB_ServiceInstall]
DisplayName     = %WinUSB_SvcDesc%
ServiceType     = 1
StartType       = 3
ErrorControl    = 1
ServiceBinary   = %12%\WinUSB.sys

[USB_Install.Wdf]
KmdfService = WINUSB, WinUSB_Install

[WinUSB_Install]
KmdfLibraryVersion  = 1.9

[USB_Install.HW]
AddReg  = Dev_AddReg

[Dev_AddReg]
HKR,,DeviceInterfaceGUIDs,0x10000,"{F72FE0D4-CBCB-407d-8814-9ED673D0DD6B}"
HKR,,DeviceIdleEnabled,0x00010001,0
HKR,,DefaultIdleState,0x00010001,0
HKR,,SystemWakeEnabled,0x00010001,0

[Strings]
ProviderName                = "Telit"
SingleAdbInterface          = "Android ADB Interface - Telit"
CompositeAdbInterface       = "Android Composite ADB Interface - Telit"
CompositeAdbInterface_cust_1054 = "SKT T-Login ADB Interface(FT980-KS)"
SingleBootLoaderInterface   = "Android Bootloader Interface"
WinUSB_SvcDesc              = "Android USB Driver"
DISK_NAME                   = "Android WinUsb installation disk"
ClassName                   = "Android Device"
