;****************************************************************
; D-Link USB 3.0 to Gigabit Ethernet Adapter
;
; Copyright 2013, D-Link Corporation
;
; Version: 1.14.7.1210	for Windows 7
;****************************************************************
[Version]
Signature  = "$Windows NT$"
CatalogFile = DUB-13X2.cat
Class      = Net
ClassGUID  = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider   = %D-Link%
DriverVer = 12/10/2012, 1.14.7.0

[Manufacturer]
%D-Link%   = USB , NTamd64.6.1

[ControlFlags]
ExcludeFromSelect = USB\VID_2001&PID_4A00

[USB.NTamd64.6.1]
%DUB-13X2.DeviceDesc% = DUB-13X2.Ndi,USB\VID_2001&PID_4A00



;****************************************************************
[DUB-13X2.Ndi]
AddReg          = DUB-13X2.Reg, DUB-13X2.Con.Reg
Characteristics = 0x84
BusType         = 15
CopyFiles       = CopyFile.Sys
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[DUB-13X2.Ndi.Services]
AddService = DUB-13X2, 2, DUB-13X2.Service, Common.EventLog

;****************************************************************
; Driver parameters
;****************************************************************

[DUB-13X2.Con.Reg]
; Connection Type
HKR,Ndi\params\*SpeedDuplex,ParamDesc,,%SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,default,,"0"
HKR,Ndi\params\*SpeedDuplex,type,,"enum"
HKR,Ndi\params\*SpeedDuplex\enum,0,,%AutoNegotiation%
HKR,Ndi\params\*SpeedDuplex\enum,1,,%10Half%
HKR,Ndi\params\*SpeedDuplex\enum,2,,%10Full%
HKR,Ndi\params\*SpeedDuplex\enum,3,,%100Half%
HKR,Ndi\params\*SpeedDuplex\enum,4,,%100Full%
HKR,Ndi\params\*SpeedDuplex\enum,6,,%1000Full%

; Mac Address
HKR,Ndi\params\NetworkAddress,ParamDesc,0,%NetworkAddress%
HKR,Ndi\params\NetworkAddress,type,0,"edit"
HKR,Ndi\params\NetworkAddress,default,0, "000000000000"
HKR,Ndi\params\NetworkAddress,LimitText,0,"12"
HKR,Ndi\params\NetworkAddress,UpperCase,0,"1"
HKR,Ndi\params\NetworkAddress,Optional,0,"1"

; Flow Control
HKR,Ndi\params\*FlowControl,ParamDesc,,%FlowControl%
HKR,Ndi\params\*FlowControl,default,,"3"
HKR,Ndi\params\*FlowControl,type,,"enum"
HKR,Ndi\params\*FlowControl\enum,0,,%Disabled%
HKR,Ndi\params\*FlowControl\enum,1,,%TxEnabled%
HKR,Ndi\params\*FlowControl\enum,2,,%RxEnabled%
HKR,Ndi\params\*FlowControl\enum,3,,%TxRxEnabled%

; Packet Priority & VLAN
HKR,Ndi\params\*PriorityVLANTag,ParamDesc,,"Packet Priority & VLAN"
HKR,Ndi\params\*PriorityVLANTag,default,,"3"
HKR,Ndi\params\*PriorityVLANTag,type,,"enum"
HKR,Ndi\params\*PriorityVLANTag\enum,0,,"Packet Priority & VLAN Disable"
HKR,Ndi\params\*PriorityVLANTag\enum,1,,"Packet Priority Enable"
HKR,Ndi\params\*PriorityVLANTag\enum,2,,"VLAN Enable"
HKR,Ndi\params\*PriorityVLANTag\enum,3,,"Packet Priority & VLAN Enable"

; Wake On Link Change
HKR,Ndi\params\WakeOnLinkChange,ParamDesc,,%WakeOnLinkChange%
HKR,Ndi\params\WakeOnLinkChange,default,,"0"
HKR,Ndi\params\WakeOnLinkChange,type,,"enum"
HKR,Ndi\params\WakeOnLinkChange\enum,0,,%Disabled%
HKR,Ndi\params\WakeOnLinkChange\enum,1,,%Enabled%

; Wake On Magic Packet
HKR,Ndi\params\*WakeOnMagicPacket,ParamDesc,,%WakeOnMagicPacket%
HKR,Ndi\params\*WakeOnMagicPacket,default,,"1"
HKR,Ndi\params\*WakeOnMagicPacket,type,,"enum"
HKR,Ndi\params\*WakeOnMagicPacket\enum,0,,%Disabled%
HKR,Ndi\params\*WakeOnMagicPacket\enum,1,,%Enabled%

; Wake On Pattern Match
HKR,Ndi\params\*WakeOnPattern,ParamDesc,,%WakeOnPattern%
HKR,Ndi\params\*WakeOnPattern,default,,"1"
HKR,Ndi\params\*WakeOnPattern,type,,"enum"
HKR,Ndi\params\*WakeOnPattern\enum,0,,%Disabled%
HKR,Ndi\params\*WakeOnPattern\enum,1,,%Enabled%

; Mask WakeUp Event Timer
HKR,Ndi\params\MaskTimer,ParamDesc,,%MaskTimer%
HKR,Ndi\params\MaskTimer,default,,"2"
HKR,Ndi\params\MaskTimer,type,,"enum"
HKR,Ndi\params\MaskTimer\enum,0,,%0sec%
HKR,Ndi\params\MaskTimer\enum,1,,%4sec%
HKR,Ndi\params\MaskTimer\enum,2,,%8sec%
HKR,Ndi\params\MaskTimer\enum,3,,%12sec%
HKR,Ndi\params\MaskTimer\enum,4,,%16sec%
HKR,Ndi\params\MaskTimer\enum,5,,%20sec%
HKR,Ndi\params\MaskTimer\enum,6,,%24sec%
HKR,Ndi\params\MaskTimer\enum,7,,%28sec%

; WOL Link Speed
HKR,Ndi\params\WolLinkSpeed,ParamDesc,,"WOL Link Power Saving"
HKR,Ndi\params\WolLinkSpeed,default,,"1"
HKR,Ndi\params\WolLinkSpeed,type,,"enum"
HKR,Ndi\params\WolLinkSpeed\enum,0,,%Disabled%
HKR,Ndi\params\WolLinkSpeed\enum,1,,%Enabled%

; TCP Checksum offload V4
HKR, Ndi\params\*TCPChecksumOffloadIPv4,ParamDesc,,"%TCPChecksumOffloadV4%"	
HKR, Ndi\params\*TCPChecksumOffloadIPv4,default,,"3"
HKR, Ndi\params\*TCPChecksumOffloadIPv4,type,0,"enum"
HKR, Ndi\params\*TCPChecksumOffloadIPv4\enum,"0",0,"%Disabled%"
HKR, Ndi\params\*TCPChecksumOffloadIPv4\enum,"1",0,"%TxEnabled%"
HKR, Ndi\params\*TCPChecksumOffloadIPv4\enum,"2",0,"%RxEnabled%"
HKR, Ndi\params\*TCPChecksumOffloadIPv4\enum,"3",0,"%TxRxEnabled%"

; UDP Checksum offload V4
HKR, Ndi\params\*UDPChecksumOffloadIPv4,ParamDesc,,"%UDPChecksumOffloadV4%"	
HKR, Ndi\params\*UDPChecksumOffloadIPv4,default,,"3"
HKR, Ndi\params\*UDPChecksumOffloadIPv4,type,0,"enum"
HKR, Ndi\params\*UDPChecksumOffloadIPv4\enum,"0",0,"%Disabled%"
HKR, Ndi\params\*UDPChecksumOffloadIPv4\enum,"1",0,"%TxEnabled%"
HKR, Ndi\params\*UDPChecksumOffloadIPv4\enum,"2",0,"%RxEnabled%"
HKR, Ndi\params\*UDPChecksumOffloadIPv4\enum,"3",0,"%TxRxEnabled%"

; TCP Checksum offload V6
HKR, Ndi\params\*TCPChecksumOffloadIPv6,ParamDesc,,"%TCPChecksumOffloadV6%"	
HKR, Ndi\params\*TCPChecksumOffloadIPv6,default,,"3"
HKR, Ndi\params\*TCPChecksumOffloadIPv6,type,0,"enum"
HKR, Ndi\params\*TCPChecksumOffloadIPv6\enum,"0",0,"%Disabled%"
HKR, Ndi\params\*TCPChecksumOffloadIPv6\enum,"1",0,"%TxEnabled%"
HKR, Ndi\params\*TCPChecksumOffloadIPv6\enum,"2",0,"%RxEnabled%"
HKR, Ndi\params\*TCPChecksumOffloadIPv6\enum,"3",0,"%TxRxEnabled%"

; UDP Checksum offload V6
HKR, Ndi\params\*UDPChecksumOffloadIPv6,ParamDesc,,"%UDPChecksumOffloadV6%"	
HKR, Ndi\params\*UDPChecksumOffloadIPv6,default,,"3"
HKR, Ndi\params\*UDPChecksumOffloadIPv6,type,0,"enum"
HKR, Ndi\params\*UDPChecksumOffloadIPv6\enum,"0",0,"%Disabled%"
HKR, Ndi\params\*UDPChecksumOffloadIPv6\enum,"1",0,"%TxEnabled%"
HKR, Ndi\params\*UDPChecksumOffloadIPv6\enum,"2",0,"%RxEnabled%"
HKR, Ndi\params\*UDPChecksumOffloadIPv6\enum,"3",0,"%TxRxEnabled%"

; IP Checksum offload V4
HKR, Ndi\params\*IPChecksumOffloadIPv4,ParamDesc,,"%IPChecksumOffloadV4%" 
HKR, Ndi\params\*IPChecksumOffloadIPv4,default,,"3"
HKR, Ndi\params\*IPChecksumOffloadIPv4,type,0,"enum"
HKR, Ndi\params\*IPChecksumOffloadIPv4\enum,"0",0,"%Disabled%"
HKR, Ndi\params\*IPChecksumOffloadIPv4\enum,"1",0,"%TxEnabled%"
HKR, Ndi\params\*IPChecksumOffloadIPv4\enum,"2",0,"%RxEnabled%"
HKR, Ndi\params\*IPChecksumOffloadIPv4\enum,"3",0,"%TxRxEnabled%"

; Large Send Offload Version 1
HKR, Ndi\params\*LsoV1IPv4,ParamDesc,,"%LsoV1IPv4%" 
HKR, Ndi\params\*LsoV1IPv4,default,,"1"
HKR, Ndi\params\*LsoV1IPv4,type,0,"enum"
HKR, Ndi\params\*LsoV1IPv4\enum,"0",0,"%Disabled%"
HKR, Ndi\params\*LsoV1IPv4\enum,"1",0,"%Enabled%"

; ARP offload
HKR,Ndi\params\*PMARPOffload,ParamDesc,,%ArpOffload%
HKR,Ndi\params\*PMARPOffload,default,,"1"
HKR,Ndi\params\*PMARPOffload,type,,"enum"
HKR,Ndi\params\*PMARPOffload\enum,0,,%Disabled%
HKR,Ndi\params\*PMARPOffload\enum,1,,%Enabled%

; NS offload
HKR,Ndi\params\*PMNSOffload,ParamDesc,,%NsOffload%
HKR,Ndi\params\*PMNSOffload,default,,"1"
HKR,Ndi\params\*PMNSOffload,type,,"enum"
HKR,Ndi\params\*PMNSOffload\enum,0,,%Disabled%
HKR,Ndi\params\*PMNSOffload\enum,1,,%Enabled%

; VLAN ID
HKR, Ndi\Params\VLAN_ID,  ParamDesc,  , %VLANID%
HKR, Ndi\Params\VLAN_ID,  Type,       , "int"
HKR, Ndi\Params\VLAN_ID,  Default,    , "0"
HKR, Ndi\params\VLAN_ID,  min,        , "0"
HKR, Ndi\params\VLAN_ID,  max,        , "4095"
HKR, Ndi\params\VLAN_ID,  step,       , "1"
HKR, NDI\params\VLAN_ID,  UpperCase,  , "1"
HKR, NDI\params\VLAN_ID,  optional,   , "1"

; Auto Detach
HKR,Ndi\params\AutoDetach,ParamDesc,,"%AutoDetach%"
HKR,Ndi\params\AutoDetach,default,,"2"
HKR,Ndi\params\AutoDetach,type,,"enum"
HKR,Ndi\params\AutoDetach\enum,0,,%Disabled%
HKR,Ndi\params\AutoDetach\enum,1,,%Enabled%
HKR,Ndi\params\AutoDetach\enum,2,,%UseEeprom%

; Wakeup Path
;HKR,Ndi\params\WakeupPath,ParamDesc,,"Wakeup Path"
;HKR,Ndi\params\WakeupPath,default,,"0"
;HKR,Ndi\params\WakeupPath,type,,"enum"
;HKR,Ndi\params\WakeupPath\enum,0,,"MAC"
;HKR,Ndi\params\WakeupPath\enum,1,,"PHY"

; Wake On External Button
;HKR,Ndi\params\WakeOnButton,ParamDesc,,"Wakeup From External Button"
;HKR,Ndi\params\WakeOnButton,default,,"0"
;HKR,Ndi\params\WakeOnButton,type,,"enum"
;HKR,Ndi\params\WakeOnButton\enum,0,,%Disabled%
;HKR,Ndi\params\WakeOnButton\enum,1,,%Enabled%

; U1/U2 Power Saving
HKR,Ndi\params\UsbPowerSave,ParamDesc,,"U1/U2 Power Saving"
HKR,Ndi\params\UsbPowerSave,default,,"0"
HKR,Ndi\params\UsbPowerSave,type,,"enum"
HKR,Ndi\params\UsbPowerSave\enum,0,,"0x00"
HKR,Ndi\params\UsbPowerSave\enum,16,,"0x10"
HKR,Ndi\params\UsbPowerSave\enum,80,,"0x50"
HKR,Ndi\params\UsbPowerSave\enum,240,,"0xF0"
HKR,Ndi\params\UsbPowerSave\enum,255,,"0xFF"

; AutoDetach Timer
HKR,Ndi\params\AutoDetachTimer,ParamDesc,,"AutoDetach Timer"
HKR,Ndi\params\AutoDetachTimer,default,,"2"
HKR,Ndi\params\AutoDetachTimer,type,,"enum"
HKR,Ndi\params\AutoDetachTimer\enum,0,,"3s"
HKR,Ndi\params\AutoDetachTimer\enum,1,,"4s"
HKR,Ndi\params\AutoDetachTimer\enum,2,,"5s"
HKR,Ndi\params\AutoDetachTimer\enum,3,,"6s"
HKR,Ndi\params\AutoDetachTimer\enum,4,,"7s"
HKR,Ndi\params\AutoDetachTimer\enum,5,,"8s"
HKR,Ndi\params\AutoDetachTimer\enum,6,,"9s"
HKR,Ndi\params\AutoDetachTimer\enum,7,,"10s"

; Phy down Timer
;HKR,Ndi\params\PhyDownTimer,ParamDesc,,"PHY Power Down Timer"
;HKR,Ndi\params\PhyDownTimer,default,,"16"
;HKR,Ndi\params\PhyDownTimer,type,,"enum"
;HKR,Ndi\params\PhyDownTimer\enum,6,,"2s"
;HKR,Ndi\params\PhyDownTimer\enum,9,,"3s"
;HKR,Ndi\params\PhyDownTimer\enum,12,,"4s"
;HKR,Ndi\params\PhyDownTimer\enum,16,,"5s"
;HKR,Ndi\params\PhyDownTimer\enum,19,,"6s"
;HKR,Ndi\params\PhyDownTimer\enum,22,,"7s"
;HKR,Ndi\params\PhyDownTimer\enum,25,,"8s"
;HKR,Ndi\params\PhyDownTimer\enum,28,,"9s"
;HKR,Ndi\params\PhyDownTimer\enum,31,,"10s"

; USB 3.0 WOL
;HKR,Ndi\params\Usb30Wol,ParamDesc,,"USB 3.0 WoL"
;HKR,Ndi\params\Usb30Wol,default,,"0"
;HKR,Ndi\params\Usb30Wol,type,,"enum"
;HKR,Ndi\params\Usb30Wol\enum,0,,%Disabled%
;HKR,Ndi\params\Usb30Wol\enum,1,,%Enabled%

; Jumbo Packet
HKR,Ndi\params\JumboPacket,ParamDesc,,"JumboPacket"
HKR,Ndi\params\JumboPacket,default,,"0"
HKR,Ndi\params\JumboPacket,type,,"enum"
HKR,Ndi\params\JumboPacket\enum,0,,%Disabled%
HKR,Ndi\params\JumboPacket\enum,1,,"2048Bytes"
HKR,Ndi\params\JumboPacket\enum,2,,"4096Bytes"

;****************************************************************
; Install section for Windows NT 5
;****************************************************************
[DUB-13X2.Reg]
; Interfaces
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi,            Service,    0, "DUB-13X2"
HKR, ,               Platform,	 0, "0"

HKR,,LogErrorMessages, 0, "1"

[DUB-13X2.Service]
DisplayName    = %DUB-13X2.DisplayName%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\DUB-13X2.sys
LoadOrderGroup = NDIS

[Common.EventLog]
AddReg = Common.AddEventLog.Reg

[Common.AddEventLog.Reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\system32\drivers\DUB-13X2.sys"
HKR, , TypesSupported  , 0x00010001, 7

[CopyFile.Sys]
DUB-13X2.sys,,,2

;**********************************************************************
; Destination directories
;**********************************************************************
[DestinationDirs]
CopyFile.Sys	= 12

[SourceDisksNames]
1=%DUB-13X2.DiskName%,,

[SourceDisksFiles]
DUB-13X2.sys=1,,

;**********************************************************************
; Localizable strings
;**********************************************************************
[Strings]
D-Link = "D-Link"
DUB-13X2.DiskName = "USB3.0 to Gigabit Ethernet Driver Diskette"
DUB-13X2.DeviceDesc = "D-Link DUB-1312/1332 USB3.0 to Gigabit Ethernet Adapter"
DUB-13X2.DisplayName = "D-Link DUB-1312/1332 USB3.0 to Gigabit Ethernet Adapter"


SpeedDuplex            = "Speed & Duplex"
AutoNegotiation        = "Auto Negotiation"
10Half                 = "10 Mbps Half Duplex"
10Full                 = "10 Mbps Full Duplex"
100Half                = "100 Mbps Half Duplex"
100Full                = "100 Mbps Full Duplex"
1000Full               = "1.0 Gbps Full Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disabled               = "Disabled"
Enabled                = "Enabled"
TxEnabled              = "Tx Enabled"
RxEnabled              = "Rx Enabled"
TxRxEnabled            = "Rx & Tx Enabled"
WakeOnLinkChange       = "Wake on link change"
WakeOnMagicPacket      = "Wake on Magic Packet"
WakeOnPattern          = "Wake on pattern match"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
LsoV1IPv4              = "Large Send Offload Version 1"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"

;Chinese_Taiwan
[Strings.0404]
D-Link = "D-Link"
DUB-13X2.DiskName = "USB3.0 to Gigabit Ethernet Driver Diskette"
DUB-13X2.DeviceDesc = "D-Link DUB-1312/1332 USB3.0 to Gigabit Ethernet Adapter"
DUB-13X2.DisplayName = "D-Link DUB-1312/1332 USB3.0 to Gigabit Ethernet Adapter"

SpeedDuplex            = "連線速度與雙工模式"
AutoNegotiation        = "自動偵測"
10Half                 = "10 Mbps 半雙工"
10Full                 = "10 Mbps 全雙工"
100Half                = "100 Mbps 半雙工"
100Full                = "100 Mbps 全雙工"
1000Full               = "1.0 Gbps 全雙工"
NetworkAddress         = "網路卡位址"
FlowControl            = "流量控制"
Disabled               = "關閉"
Enabled                = "開啟"
TxEnabled              = "Tx 開啟"
RxEnabled              = "Rx 開啟"
TxRxEnabled             = "Rx & Tx 開啟"
WakeOnLinkChange       = "網路連接喚醒"
WakeOnMagicPacket      = "魔術封包"
WakeOnPattern          = "喚醒封包"
VLANID                 = "虛擬區域網路編號"
TCPChecksumOffloadV4   = "TCP 檢查總和卸載 (IPv4)"
UDPChecksumOffloadV4   = "UDP 檢查總和卸載 (IPv4)"
TCPChecksumOffloadV6   = "TCP 檢查總和卸載 (IPv6)"
UDPChecksumOffloadV6   = "UDP 檢查總和卸載 (IPv6)"
IPChecksumOffloadV4    = "IPv4 檢查總和值卸載"
LsoV1IPv4              = "大量傳送卸載 V1 (IPv4)"
ARPOffload             = "ARP 卸載"
NsOffload              = "NS 卸載"
AutoDetach             = "自動卸載"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL 連線速度"
10mFirst               = "10 Mbps First"
MaskTimer              = "遮蔽喚醒事件計時器"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"

;Chinese_PRC
[Strings.0804]
D-Link = "D-Link"
DUB-13X2.DiskName = "USB3.0 to Gigabit Ethernet Driver Diskette"
DUB-13X2.DeviceDesc = "D-Link DUB-1312/1332 USB3.0 to Gigabit Ethernet Adapter"
DUB-13X2.DisplayName = "D-Link DUB-1312/1332 USB3.0 to Gigabit Ethernet Adapter"

SpeedDuplex            = "连接速度和双工模式"
AutoNegotiation        = "自动检测"
10Half                 = "10 Mbps半双工"
10Full                 = "10 Mbps全双工"
100Half                = "100 Mbps半双工"
100Full                = "100 Mbps全双工"
1000Full               = "1.0 Gbps全双工"
NetworkAddress         = "网络地址"
FlowControl            = "流量控制"
Disabled               = "禁用"
Enabled                = "启用"
TxEnabled              = "Tx 启用"
RxEnabled              = "Rx 启用"
TxRxEnabled            = "Rx & Tx 启用"
WakeOnLinkChange       = "网络连接唤醒"
WakeOnMagicPacket      = "魔术包唤醒"
WakeOnPattern          = "唤醒帧唤醒"
VLANID                 = "VLAN标识"
TCPChecksumOffloadV4   = "TCP校验和承载(IPv4)"
UDPChecksumOffloadV4   = "UDP校验和承载(IPv4)"
TCPChecksumOffloadV6   = "TCP校验和承载(IPv6)"
UDPChecksumOffloadV6   = "UDP校验和承载(IPv6)"
IPChecksumOffloadV4    = "IPv4校验和承载"
LsoV1IPv4              = "大量传送负载V1(IPv4)"
ARPOffload             = "ARP承载"
NsOffload              = "NS承载"
AutoDetach             = "自动分离（卸载）"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL链接速率"
10mFirst               = "10 Mbps First"
MaskTimer              = "屏蔽唤醒事件定时器"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"

;Japanese
[Strings.0411]
D-Link = "D-Link"
DUB-13X2.DiskName = "USB3.0 to Gigabit Ethernet Driver Diskette"
DUB-13X2.DeviceDesc = "D-Link DUB-1312/1332 USB3.0 to Gigabit Ethernet Adapter"
DUB-13X2.DisplayName = "D-Link DUB-1312/1332 USB3.0 to Gigabit Ethernet Adapter"

SpeedDuplex	       = "速度とデュプレックス"
AutoNegotiation        = "自動認識"
10Half                 = "10 Mbps 半二重"
10Full                 = "10 Mbps 全二重"
100Half                = "100 Mbps 半二重"
100Full                = "100 Mbps 全二重"
1000Full               = "1.0 Gbps 全二重"
NetworkAddress         = "ネットワークアドレス"
FlowControl            = "帯域制御"
Disabled               = "無効"
Enabled                = "有効"
TxEnabled              = "Tx 有効"
RxEnabled              = "Rx 有効"
TxRxEnabled            = "Rx & Tx 有効"
WakeOnLinkChange       = "ウェイクオン・リンク変化"
WakeOnMagicPacket      = "ウェイクオン・マジックパケット"
WakeOnPattern          = "ウェイクオン・パターン"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCPチェックサム・オフロード(IPv4)"
UDPChecksumOffloadV4   = "UDPチェックサム・オフロード(IPv4)"
TCPChecksumOffloadV6   = "TCPチェックサム・オフロード(IPv6)"
UDPChecksumOffloadV6   = "UDPチェックサム・オフロード(IPv6)"
IPChecksumOffloadV4    = "IPv4 チェックサム・オフロード"
LsoV1IPv4              = "Large Send Offload Version 1"
ARPOffload             = "ARPオフロード"
NsOffload              = "NSオフロード"
AutoDetach             = "自動切り離し"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL リンクスピード"
10mFirst               = "10 Mbps First"
MaskTimer              = "マスク時間"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"

;Korean
[Strings.0412]
D-Link = "D-Link"
DUB-13X2.DiskName = "USB3.0 to Gigabit Ethernet Driver Diskette"
DUB-13X2.DeviceDesc = "D-Link DUB-1312/1332 USB3.0 to Gigabit Ethernet Adapter"
DUB-13X2.DisplayName = "D-Link DUB-1312/1332 USB3.0 to Gigabit Ethernet Adapter"

SpeedDuplex            = "속도 및 이중"
AutoNegotiation        = "자동감지"
10Half                 = "10 Mbps 반이중"
10Full                 = "10 Mbps 전이중"
100Half                = "100 Mbps 반이중"
100Full                = "100 Mbps 전이중"
1000Full               = "1.0 Gbps 전이중"
NetworkAddress         = "네트워크 주소"
FlowControl            = "흐름 제어"
Disabled               = "사용 않함"
Enabled                = "사용"
TxEnabled              = "Tx 사용"
RxEnabled              = "Rx 사용"
TxRxEnabled            = "Rx & Tx 사용"
WakeOnLinkChange       = "Wake on link change"
WakeOnMagicPacket      = "Wake on Magic Packet"
WakeOnPattern          = "Wake on pattern match"
VLANID                 = "VLAN 아이디"
TCPChecksumOffloadV4   = "TCP 체크섬 오프로드 (IPv4)"
UDPChecksumOffloadV4   = "UDP 체크섬 오프로드 (IPv4)"
TCPChecksumOffloadV6   = "TCP 체크섬 오프로드 (IPv6)"
UDPChecksumOffloadV6   = "UDP 체크섬 오프로드 (IPv4)"
IPChecksumOffloadV4    = "IPv4 체크섬 오프로드"
LsoV1IPv4              = "LSO(Large Send Offload) v1 (IPv4)"
ARPOffload             = "Arp 오프로드"
NsOffload              = "NS 오프로드"
AutoDetach             = "자동 제거"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL 연결 속도 변경"
10mFirst               = "10 Mbps First"
MaskTimer              = "WOL 이벤트 차단 시간"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"

[Strings.0407]
D-Link = "D-Link"
DUB-13X2.DiskName = "USB3.0 to Gigabit Ethernet Driver Diskette"
DUB-13X2.DeviceDesc = "D-Link DUB-1312/1332 USB3.0 to Gigabit Ethernet Adapter"
DUB-13X2.DisplayName = "D-Link DUB-1312/1332 USB3.0 to Gigabit Ethernet Adapter"

SpeedDuplex            = "Geschwindigkeit & Duplex"
AutoNegotiation        = "Auto Negotiation"
10Half                 = "10 Mbps Half Duplex"
10Full                 = "10 Mbps Full Duplex"
100Half                = "100 Mbps Half Duplex"
100Full                = "100 Mbps Full Duplex"
1000Full               = "1.0 Gbps Full Duplex"
NetworkAddress         = "Netzwerkadresse"
FlowControl            = "Flow Control"
Disabled               = "Ausgeschaltet"
Enabled                = "Eingeschaltet"
TxEnabled              = "Tx Eingeschaltet"
RxEnabled              = "Rx Eingeschaltet"
TxRxEnabled            = "Rx & Tx Eingeschaltet"
WakeOnLinkChange       = "Wake on link change"
WakeOnMagicPacket      = "Wake on Magic Packet"
WakeOnPattern          = "Wake on pattern match"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
LsoV1IPv4              = "Abladung großer ÜbertragungV1(IPv4)"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"

[Strings.0419]
D-Link = "D-Link"
DUB-13X2.DiskName = "USB3.0 to Gigabit Ethernet Driver Diskette"
DUB-13X2.DeviceDesc = "D-Link DUB-1312/1332 USB3.0 to Gigabit Ethernet Adapter"
DUB-13X2.DisplayName = "D-Link DUB-1312/1332 USB3.0 to Gigabit Ethernet Adapter"

SpeedDuplex            = "Скорость и дуплекс"
AutoNegotiation        = "Автопереговоры"
10Half                 = "10 Мбит/сек полудуплекс"
10Full                 = "10 Мбит/сек полный дуплекс"
100Half                = "100 Мбит/сек полудуплекс"
100Full                = "100 Мбит/сек полный дуплекс"
1000Full               = "1.0 Гбит/сек полный дуплекс"
NetworkAddress         = "Сетевой адрес"
FlowControl            = "Управление потоком"
Disabled               = "Запрещен"
Enabled                = "Разрешен"
TxEnabled              = "Передача разрешена"
RxEnabled              = "Прием разрешен"
TxRxEnabled            = "Прием и передача разрешены"
WakeOnLinkChange       = "Wake on link change"
WakeOnMagicPacket      = "Wake on Magic Packet"
WakeOnPattern          = "Wake on pattern match"
VLANID                 = "VLAN ID"
TCPChecksumOffloadV4   = "TCP Checksum Offload (IPv4)"
UDPChecksumOffloadV4   = "UDP Checksum Offload (IPv4)"
TCPChecksumOffloadV6   = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadV6   = "UDP Checksum Offload (IPv6)"
IPChecksumOffloadV4    = "IPv4 Checksum Offload"
LsoV1IPv4              = "Large Send Offload Version 1"
ARPOffload             = "ARP Offload"
NsOffload              = "NS Offload"
AutoDetach             = "AutoDetach"
UseEeprom              = "Use EEPROM Setting"
WolLinkSpeed           = "WOL Link Speed"
10mFirst               = "10 Mbps First"
MaskTimer              = "Mask WakeUp Event Timer"
0sec                   = "0 second"
4sec                   = "4 seconds"
8sec                   = "8 seconds"
12sec                  = "12 seconds"
16sec                  = "16 seconds"
20sec                  = "20 seconds"
24sec                  = "24 seconds"
28sec                  = "28 seconds"
