;   Prolific PL2303G VCP / PL232X CDC Series

;   plser_1.INF (for Win11)

;   Copyright (c) 2021, Prolific Technology Inc.



[version]
signature="$CHICAGO$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%PRO%
DriverVer=11/06/2025,5.2.10.2
PnpLockdown=1
CatalogFile=plser_1.cat

; ================= Device Install section =====================

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%PRO%=PRO,NTAMD64

[SourceDisksNames]
1=%DISK_NAME%,

[SourceDisksFiles]
plser64_1.sys = 1

[DestinationDirs] 
DefaultDestDir  = 12

[PRO.NTAMD64]
%DeviceDesc1% = ComPort, USB\VID_067B&PID_23B3
%DeviceDesc2% = ComPort, USB\VID_067B&PID_23C3
%DeviceDesc3% = ComPort, USB\VID_067B&PID_23D3
%DeviceDesc4% = ComPort, USB\VID_067B&PID_23E3
%DeviceDesc5% = ComPort, USB\VID_067B&PID_23F3
%DeviceDesc6% = ComPort, USB\VID_067B&PID_2323
%DeviceDesc7% = ComPort, USB\VID_067B&PID_23A3&REV_0805
%DeviceDesc8% = ComPort, USB\VID_067B&PID_23A3&REV_0705
%DeviceDesc9% = ComPort, USB\VID_067B&PID_23A3&REV_0605
%DeviceDesc10% = ComPort, USB\VID_067B&PID_23A3&REV_0505
%DeviceDesc11% = ComPort, USB\VID_067B&PID_23A3&REV_0405
%DeviceDesc12% = ComPort, USB\VID_067B&PID_23A3&REV_0305
%DeviceDesc13% = ComPort, USB\VID_067B&PID_23A3&REV_0105
%DeviceDesc14% = ComPort, USB\VID_067B&PID_23A3&REV_0100
%DeviceDesc15% = ComPort, USB\VID_067B&PID_23A3&REV_0700
%DeviceDesc16% = ComPort, USB\VID_067B&PID_23A3
%DeviceDesc17% = ComPort, USB\VID_067B&PID_FFFF
%DeviceDesc18% = ComPort, USB\VID_067B&PID_2320
%DeviceDesc19% = ComPort, USB\VID_067B&PID_2321&MI_00
%DeviceDesc20% = ComPort, USB\VID_067B&PID_2322
%DeviceDesc21% = ComPort, USB\VID_067B&PID_23A3&REV_0905
%DeviceDesc22% = ComPort, USB\VID_067B&PID_23A3&REV_1005
%DeviceDesc23% = ComPort, USB\VID_067B&PID_23A3&REV_1105
%DeviceDesc24% = ComPort, USB\VID_067B&PID_23A3&REV_1205

[ComPort.HW.AddReg]
HKR,,"UpperFilters",0x00010000,"serenum"
HKR,,"PL2303C1",0x00010001,10
HKR,,"PL2303C2",0x00010001,0
HKR,,"PL2303C3",0x00010001,4096

[ComPort.NTAMD64]
CopyFiles=ComPort.NTAMD64.Copy
AddReg=ComPort.NTAMD64.AddReg

[ComPort.NTAMD64.HW]
AddReg=ComPort.HW.AddReg

[ComPort.NTAMD64.Services]
AddService = plser, 0x00000002, Serial_Service_Inst.NTAMD64

[ComPort.NTAMD64.Copy]
plser64_1.sys

[ComPort.NTAMD64.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,plser64_1.sys
HKR,,NTMPDriver,,serenum.sys
HKR,,PortSubClass,1,01
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[Serial_Service_Inst.NTAMD64]
DisplayName    = %Serial.SVCDESC%                            
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\plser64_1.sys                            
LoadOrderGroup = Base


[Strings]
PRO = "Prolific"
DeviceDesc1 = "Prolific PL2303GB USB Serial COM Port"
DeviceDesc2 = "Prolific PL2303GT USB Serial COM Port"
DeviceDesc3 = "Prolific PL2303GL USB Serial COM Port"
DeviceDesc4 = "Prolific PL2303GE USB Serial COM Port"
DeviceDesc5 = "Prolific PL2303GS USB Serial COM Port"
DeviceDesc6 = "Prolific PL2303GD USB Serial COM Port"
DeviceDesc7 = "Prolific PL2303GD USB Serial COM Port"
DeviceDesc8 = "Prolific PL2303GR USB Serial COM Port"
DeviceDesc9 = "Prolific PL2303GS USB Serial COM Port"
DeviceDesc10 = "Prolific PL2303GE USB Serial COM Port"
DeviceDesc11 = "Prolific PL2303GL USB Serial COM Port"
DeviceDesc12 = "Prolific PL2303GT USB Serial COM Port"
DeviceDesc13 = "Prolific PL2303GC USB Serial COM Port"
DeviceDesc14 = "Prolific PL2303GC USB Serial COM Port"
DeviceDesc15 = "Prolific PL2303GD USB Serial COM Port"
DeviceDesc16 = "Prolific PL2303GC USB Serial COM Port"
DeviceDesc17 = "Prolific PL2303FF USB Serial COM Port"
DeviceDesc18 = "Prolific PL2320 USB CDC Serial Port"
DeviceDesc19 = "Prolific PL2321 USB CDC Serial Port"
DeviceDesc20 = "Prolific PL2322 USB CDC Serial Port"
DeviceDesc21 = "Prolific PL2303GT USB Serial COM Port"
DeviceDesc22 = "Prolific PL2303GC USB Serial COM Port"
DeviceDesc23 = "Prolific PL2303G USB Serial COM Port"
DeviceDesc24 = "Prolific PL2303G USB Serial COM Port"
Serial.SVCDESC  = "Prolific PLSER Serial Port WDF Driver"
DISK_NAME = "USB-Serial Cable Diskette"
